|  |  |
| --- | --- |
| **In FVCOM41\_source:** | |
|  | |
| **Modified (3):** | |
| ice\_flux\_in.F | Fixed a bug via adding 'use mod\_utils, only: Fatal\_Error' in subroutine prepare\_forcing |
| mod\_non\_hydro.F | Added the subroutine calls to new version of PETSc (missed in FVCOM 4.0) |
| mod\_setup.F | Fixed a bug in subroutine SETUP\_CENTER\_COORDS:  call ADEAL(MYID,MSRID,NPROCS,EXMAP,xc\_buf,ymc) => call ADEAL(MYID,MSRID,NPROCS,EXMAP,yc\_buf,ymc) |